AS01-ASBR01
Current configuration : 8233 bytes
!
! Last configuration change at 08:26:15 UTC Wed Aug 28 2024
!
version 17.3
service timestamps debug datetime msec
service timestamps log datetime msec
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
platform console serial
!
hostname AS01-ASBR01
!
boot-start-marker
boot-end-marker
!
!
vrf definition LAB009
 rd 9:1
 !
 address-family ipv4
  route-target export 9:1
  route-target import 9:1
 exit-address-family
!
no logging console
!
no aaa new-model
!
!
!
!
!
!
!
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
! 
! 
! 
! 
!
!
mpls ldp label
 allocate global host-routes
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
crypto pki trustpoint TP-self-signed-3683107136
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-3683107136
 revocation-check none
 rsakeypair TP-self-signed-3683107136
!
!
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030 
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363 
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934 
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305 
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720 
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030 
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D 
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520 
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE 
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC 
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188 
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7 
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191 
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44 
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201 
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85 
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500 
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905 
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B 
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8 
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C 
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B 
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678 
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB 
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0 
  D697DF7F 28
  quit
crypto pki certificate chain TP-self-signed-3683107136
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030 
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274 
  69666963 6174652D 33363833 31303731 3336301E 170D3233 30363133 31343138 
  31315A17 0D333330 36313231 34313831 315A3031 312F302D 06035504 03132649 
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D33 36383331 
  30373133 36308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201 
  0A028201 0100B19E FD77ABB7 3F5C234B 9275F018 A342F36A A1867088 B8593780 
  34CCB010 87D1A286 DE88E734 E42B458A BFDCAAA1 4C660491 84DAD18B 81D98CCF 
  9E47F7EB C16FA29E 0EE45E1D A0900718 AF214075 BC980A08 AAF7316B E6702AE2 
  D6C36DA5 CF57A365 7B965DE5 75745EC4 8CA59C5B 4A455170 27B90005 41C28054 
  AC7595B3 F24837D6 71F25AAB C6347C24 8EAF23F2 2EF226F0 FC4A7610 5F1ED0E5 
  1702D742 F1C28F04 48E6B548 83F91FFF E4CAB8D1 E6F4D1C0 6E58BA33 5A89C710 
  55CA9EC6 F6F41D47 D5399B54 B14E0C78 F7BEF216 4E01D55B 02E0DB99 8FD27F1D 
  34331E20 0D440EAE 49A65660 E5EDF5FD F680977A 4D3F7FFF F5A41D3E 18603243 
  5EC1FE4C 9CFF0203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF 
  301F0603 551D2304 18301680 14702BF3 6DFFBA37 93EC5FC3 8F1E387E 67293502 
  CA301D06 03551D0E 04160414 702BF36D FFBA3793 EC5FC38F 1E387E67 293502CA 
  300D0609 2A864886 F70D0101 05050003 82010100 46C2CC7E 85C50CCB 04DAA109 
  E523D922 6944CE88 FEF5D695 DFEEF655 CF53C319 5645149F E644D7D2 39019D48 
  DA131A85 A8814478 EE09C587 74B1A493 5DB3968C D28F9E39 E1DA4CC0 A8950E0E 
  C20C32E9 CF0DDF70 C1240CEC 8AC7B799 128F8921 2B232F46 1DEFE8A2 207C573C 
  01150343 F6F2A583 E6F456D3 8E81B855 799A60BC 0CEF428E E1045F7B 9C25765F 
  00493E63 748A63BA DD8F0F0B 86F800ED 1FA84684 22CF4736 9A50E469 EE8FA3B3 
  79A3CA5B 88E9C288 819310D9 462A438B 7178B881 4E802B5E CC1699F3 1F90D04D 
  37D4F91E A49C1293 64575736 03FED133 709EFA72 E1D0496D 8A27B8F0 4574894E 
  B2F4EA5D DBA16629 B274CECF 90E81AEC 3CA58EE1
  quit
!
license udi pid CSR1000V sn 9DKZS7A1DMX
diagnostic bootup level minimal
memory free low-watermark processor 71489
!
!
spanning-tree extend system-id
!
!
redundancy
!
!
!
!
!
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
!
! 
! 
!
!
interface Loopback0
 ip address 172.17.0.200 255.255.255.255
!
interface GigabitEthernet1
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 81 ethernet
  encapsulation dot1q 81
  rewrite ingress tag pop 1 symmetric
  xconnect 172.17.0.50 81 encapsulation mpls
 !
 service instance 82 ethernet
  encapsulation dot1q 82
  rewrite ingress tag pop 1 symmetric
  xconnect 172.17.0.40 82 encapsulation mpls
 !
 service instance 91 ethernet
  encapsulation dot1q 91
  rewrite ingress tag pop 1 symmetric
  bridge-domain 91
 !
 service instance 101 ethernet
  encapsulation dot1q 101
  rewrite ingress tag pop 1 symmetric
  bridge-domain 101
 !
 service instance 111 ethernet
  encapsulation dot1q 111
  rewrite ingress tag pop 1 symmetric
 !
!
interface GigabitEthernet2
 no ip address
 shutdown
 negotiation auto
 no mop enabled
 no mop sysid
!
interface GigabitEthernet3
 ip address 172.16.200.2 255.255.255.0
 negotiation auto
 mpls ip
 no mop enabled
 no mop sysid
!
interface GigabitEthernet4
 no ip address
 shutdown
 negotiation auto
 no mop enabled
 no mop sysid
!
interface BDI91
 vrf forwarding LAB009
 ip address 91.0.0.1 255.255.255.0
 no mop enabled
 no mop sysid
!
interface BDI101
 ip address 101.0.0.1 255.255.255.0
 mpls ip
 no mop enabled
 no mop sysid
!
interface BDI111
 ip address 111.0.0.1 255.255.255.0
 shutdown
 no mop enabled
 no mop sysid
!
router ospf 1
 network 101.0.0.0 0.0.0.255 area 0
 network 172.16.0.0 0.0.255.255 area 0
 network 172.17.0.0 0.0.0.255 area 0
!
router bgp 1
 bgp log-neighbor-changes
 no bgp default ipv4-unicast
 no bgp default route-target filter
 neighbor 101.0.0.2 remote-as 2
 neighbor 101.0.0.2 ebgp-multihop 255
 neighbor 172.17.0.100 remote-as 1
 neighbor 172.17.0.100 update-source Loopback0
 !
 address-family ipv4
  neighbor 172.17.0.100 activate
 exit-address-family
 !
 address-family vpnv4
  neighbor 172.17.0.100 activate
  neighbor 172.17.0.100 send-community both
 exit-address-family
 !
 address-family l2vpn vpls
  neighbor 101.0.0.2 activate
  neighbor 101.0.0.2 send-community both
  neighbor 101.0.0.2 next-hop-self
  neighbor 172.17.0.100 activate
  neighbor 172.17.0.100 send-community both
  neighbor 172.17.0.100 next-hop-self
 exit-address-family
 !
 address-family ipv4 vrf LAB009
  neighbor 91.0.0.2 remote-as 2
  neighbor 91.0.0.2 activate
 exit-address-family
!
ip forward-protocol nd
no ip http server
ip http secure-server
!
!
!
!
!
!
!
!
control-plane
!
!
!
!
!
!
line con 0
 exec-timeout 0 0
 stopbits 1
line vty 0
 exec-timeout 0 0
 login
 transport input ssh
line vty 1
 exec-timeout 0 0
 login
 length 0
 transport input ssh
line vty 2 4
 exec-timeout 0 0
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
end

##################################################################################

AS01-CE01
Current configuration : 4029 bytes
!
! Last configuration change at 13:46:57 UTC Mon Aug 26 2024
!
version 15.9
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname AS01-CE01
!
boot-start-marker
boot-end-marker
!
!
vrf list 121
!
no logging console
!
no aaa new-model
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
ip vrf 1121
 rd 1:121
!
ip vrf 121
 rd 1:21
!
ip vrf 122
 rd 1:22
!
ip vrf 131
 rd 1:31
!
ip vrf 141
 rd 1:41
!
!
!
!
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
redundancy
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/1.121
 encapsulation dot1Q 121
 ip vrf forwarding 121
 ip address 10.1.2.1 255.0.0.0
!
interface GigabitEthernet0/2
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/3
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/3.122
 encapsulation dot1Q 122
 ip vrf forwarding 122
 ip address 10.1.2.2 255.0.0.0
!
interface GigabitEthernet0/4
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/4.131
 encapsulation dot1Q 131
 ip vrf forwarding 131
 ip address 10.1.3.1 255.0.0.0
!
interface GigabitEthernet0/5
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/5.141
 encapsulation dot1Q 141
 ip vrf forwarding 141
 ip address 10.1.4.1 255.0.0.0
!
interface GigabitEthernet0/6
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/6.1121
 encapsulation dot1Q 1121
 ip vrf forwarding 1121
 ip address 10.1.12.1 255.0.0.0
!
interface GigabitEthernet0/7
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 ioam timestamp
!
!
!
control-plane
!
banner exec <
>
!
line con 0
 exec-timeout 0 0
line aux 0
line vty 0 4
 exec-timeout 0 0
 login
 transport input none
!
no scheduler allocate
!
end

##################################################################################

AS01-CE02
Current configuration : 3827 bytes
!
version 15.9
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname AS01-CE02
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
ip vrf 231
 rd 2:31
!
ip vrf 241
 rd 2:41
!
ip vrf 261
 rd 2:61
!
ip vrf 271
 rd 2:71
!
!
!
!
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
redundancy
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/1.231
 encapsulation dot1Q 231
 ip vrf forwarding 231
 ip address 10.2.3.1 255.0.0.0
!
interface GigabitEthernet0/2
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/2.241
 encapsulation dot1Q 241
 ip vrf forwarding 241
 ip address 10.2.4.1 255.0.0.0
!
interface GigabitEthernet0/3
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/4
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/4.261
 encapsulation dot1Q 261
 ip vrf forwarding 261
 ip address 10.2.6.1 255.0.0.0
!
interface GigabitEthernet0/5
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/5.271
 encapsulation dot1Q 271
 ip vrf forwarding 271
 ip address 10.2.7.1 255.0.0.0
!
interface GigabitEthernet0/6
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/7
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 ioam timestamp
!
!
!
control-plane
!
banner exec <
>
!
line con 0
 exec-timeout 0 0
line aux 0
line vty 0 4
 exec-timeout 0 0
 login
 transport input none
!
no scheduler allocate
!
end

##################################################################################

AS01-CE03
Current configuration : 3827 bytes
!
version 15.9
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname AS01-CE03
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
ip vrf 331
 rd 3:31
!
ip vrf 341
 rd 3:41
!
ip vrf 361
 rd 3:61
!
ip vrf 371
 rd 3:71
!
!
!
!
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
redundancy
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/1.331
 encapsulation dot1Q 331
 ip vrf forwarding 331
 ip address 10.3.3.1 255.0.0.0
!
interface GigabitEthernet0/2
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/3
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/3.341
 encapsulation dot1Q 341
 ip vrf forwarding 341
 ip address 10.3.4.1 255.0.0.0
!
interface GigabitEthernet0/4
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/4.361
 encapsulation dot1Q 361
 ip vrf forwarding 361
 ip address 10.3.6.1 255.0.0.0
!
interface GigabitEthernet0/5
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/5.371
 encapsulation dot1Q 371
 ip vrf forwarding 371
 ip address 10.3.7.1 255.0.0.0
!
interface GigabitEthernet0/6
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/7
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 ioam timestamp
!
!
!
control-plane
!
banner exec <
>
!
line con 0
 exec-timeout 0 0
line aux 0
line vty 0 4
 exec-timeout 0 0
 login
 transport input none
!
no scheduler allocate
!
end

##################################################################################

AS01-CE04
Current configuration : 4087 bytes
!
version 15.9
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname AS01-CE04
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
ip vrf 4121
 rd 4:121
!
ip vrf 421
 rd 4:21
!
ip vrf 422
 rd 4:22
!
ip vrf 431
 rd 4:31
!
ip vrf 441
 rd 4:41
!
ip vrf 481
 rd 4:81
!
!
!
!
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
redundancy
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/0.422
 encapsulation dot1Q 422
 ip vrf forwarding 422
 ip address 10.4.2.2 255.0.0.0
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/1.421
 encapsulation dot1Q 421
 ip vrf forwarding 421
 ip address 10.4.2.1 255.0.0.0
!
interface GigabitEthernet0/2
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/2.431
 encapsulation dot1Q 431
 ip vrf forwarding 431
 ip address 10.4.3.1 255.0.0.0
!
interface GigabitEthernet0/3
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/4
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/4.441
 encapsulation dot1Q 441
 ip vrf forwarding 441
 ip address 10.4.4.1 255.0.0.0
!
interface GigabitEthernet0/5
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/5.481
 encapsulation dot1Q 481
 ip vrf forwarding 481
 ip address 10.4.8.1 255.0.0.0
!
interface GigabitEthernet0/6
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/6.4121
 encapsulation dot1Q 412
 ip vrf forwarding 4121
 ip address 10.4.12.1 255.0.0.0
!
interface GigabitEthernet0/7
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 ioam timestamp
!
!
!
control-plane
!
banner exec <
>
!
line con 0
 exec-timeout 0 0
line aux 0
line vty 0 4
 exec-timeout 0 0
 login
 transport input none
!
no scheduler allocate
!
end

##################################################################################

AS01-CE05
Current configuration : 3965 bytes
!
version 15.9
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname AS01-CE05
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
ip vrf 5101
 rd 5:101
!
ip vrf 5121
 rd 5:121
!
ip vrf 561
 rd 5:61
!
ip vrf 571
 rd 5:71
!
ip vrf 581
 rd 5:81
!
!
!
!
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
redundancy
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/1.561
 encapsulation dot1Q 561
 ip vrf forwarding 561
 ip address 10.5.6.1 255.0.0.0
!
interface GigabitEthernet0/2
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/3
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/3.571
 encapsulation dot1Q 571
 ip vrf forwarding 571
 ip address 10.5.7.1 255.0.0.0
!
interface GigabitEthernet0/4
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/4.581
 encapsulation dot1Q 581
 ip vrf forwarding 581
 ip address 10.5.8.1 255.0.0.0
!
interface GigabitEthernet0/5
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/5.511
 encapsulation dot1Q 511
 ip vrf forwarding 5101
 ip address 10.5.10.1 255.0.0.0
!
interface GigabitEthernet0/6
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/6.5121
 encapsulation dot1Q 512
 ip vrf forwarding 5121
 ip address 10.5.12.1 255.0.0.0
!
interface GigabitEthernet0/7
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 ioam timestamp
!
!
!
control-plane
!
banner exec <
>
!
line con 0
 exec-timeout 0 0
line aux 0
line vty 0 4
 exec-timeout 0 0
 login
 transport input none
!
no scheduler allocate
!
end

##################################################################################

AS01-CE06
Current configuration : 4011 bytes
!
version 15.9
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname AS01-CE06
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
ip vrf 6111
 rd 6:111
!
ip vrf 6121
 rd 6:121
!
ip vrf 661
 rd 6:61
!
ip vrf 671
 rd 6:71
!
ip vrf 691
 rd 6:91
!
!
!
!
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
redundancy
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/1.661
 encapsulation dot1Q 661
 ip vrf forwarding 661
 ip address 10.6.6.1 255.0.0.0
!
interface GigabitEthernet0/2
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/3
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/3.671
 encapsulation dot1Q 671
 ip vrf forwarding 671
 ip address 10.6.7.1 255.0.0.0
!
interface GigabitEthernet0/4
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/4.691
 encapsulation dot1Q 691
 ip vrf forwarding 691
 ip address 10.6.9.1 255.255.255.0
!
interface GigabitEthernet0/5
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/5.611
 encapsulation dot1Q 611
 ip vrf forwarding 6111
 ip address 10.6.11.1 255.0.0.0
!
interface GigabitEthernet0/6
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/6.6121
 encapsulation dot1Q 621
 ip vrf forwarding 6121
 ip address 10.6.12.1 255.0.0.0
!
interface GigabitEthernet0/7
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
ip route vrf 691 0.0.0.0 0.0.0.0 10.6.9.2
!
ipv6 ioam timestamp
!
!
!
control-plane
!
banner exec <
>
!
line con 0
 exec-timeout 0 0
line aux 0
line vty 0 4
 exec-timeout 0 0
 login
 transport input none
!
no scheduler allocate
!
end

##################################################################################

AS01-P01
Current configuration : 3465 bytes
!
version 15.9
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname AS01-P01
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
mpls traffic-eng tunnels
!
!
!
!
!
redundancy
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 172.17.0.1 255.255.255.255
!
interface GigabitEthernet0/0
 ip address 172.16.0.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls traffic-eng tunnels
 mpls ip
 ip rsvp bandwidth
!
interface GigabitEthernet0/1
 ip address 172.16.3.2 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls traffic-eng tunnels
 mpls ip
 ip rsvp bandwidth
!
interface GigabitEthernet0/2
 ip address 172.16.50.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls traffic-eng tunnels
 mpls ip
 ip rsvp bandwidth
!
interface GigabitEthernet0/3
 ip address 172.16.100.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls traffic-eng tunnels
 mpls ip
 ip rsvp bandwidth
!
router ospf 1
 mpls traffic-eng router-id Loopback0
 mpls traffic-eng area 0
 network 172.16.0.0 0.0.255.255 area 0
 network 172.17.0.0 0.0.0.255 area 0
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 ioam timestamp
!
!
!
control-plane
!
banner exec <
>
!
line con 0
 exec-timeout 0 0
line aux 0
line vty 0 4
 exec-timeout 0 0
 login
 transport input none
!
no scheduler allocate
!
end

##################################################################################

AS01-P02
Current configuration : 3465 bytes
!
version 15.9
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname AS01-P02
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
mpls traffic-eng tunnels
!
!
!
!
!
redundancy
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 172.17.0.2 255.255.255.255
!
interface GigabitEthernet0/0
 ip address 172.16.0.2 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls traffic-eng tunnels
 mpls ip
 ip rsvp bandwidth
!
interface GigabitEthernet0/1
 ip address 172.16.1.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls traffic-eng tunnels
 mpls ip
 ip rsvp bandwidth
!
interface GigabitEthernet0/2
 ip address 172.16.60.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls traffic-eng tunnels
 mpls ip
 ip rsvp bandwidth
!
interface GigabitEthernet0/3
 ip address 172.16.200.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls traffic-eng tunnels
 mpls ip
 ip rsvp bandwidth
!
router ospf 1
 mpls traffic-eng router-id Loopback0
 mpls traffic-eng area 0
 network 172.16.0.0 0.0.255.255 area 0
 network 172.17.0.0 0.0.0.255 area 0
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 ioam timestamp
!
!
!
control-plane
!
banner exec <
>
!
line con 0
 exec-timeout 0 0
line aux 0
line vty 0 4
 exec-timeout 0 0
 login
 transport input none
!
no scheduler allocate
!
end

##################################################################################

AS01-P03
Current configuration : 3464 bytes
!
version 15.9
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname AS01-P03
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
mpls traffic-eng tunnels
!
!
!
!
!
redundancy
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 172.17.0.3 255.255.255.255
!
interface GigabitEthernet0/0
 ip address 172.16.2.2 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls traffic-eng tunnels
 mpls ip
 ip rsvp bandwidth
!
interface GigabitEthernet0/1
 ip address 172.16.3.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls traffic-eng tunnels
 mpls ip
 ip rsvp bandwidth
!
interface GigabitEthernet0/2
 ip address 172.16.10.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls traffic-eng tunnels
 mpls ip
 ip rsvp bandwidth
!
interface GigabitEthernet0/3
 ip address 172.16.20.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls traffic-eng tunnels
 mpls ip
 ip rsvp bandwidth
!
router ospf 1
 mpls traffic-eng router-id Loopback0
 mpls traffic-eng area 0
 network 172.16.0.0 0.0.255.255 area 0
 network 172.17.0.0 0.0.0.255 area 0
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 ioam timestamp
!
!
!
control-plane
!
banner exec <
>
!
line con 0
 exec-timeout 0 0
line aux 0
line vty 0 4
 exec-timeout 0 0
 login
 transport input none
!
no scheduler allocate
!
end

##################################################################################

AS01-P04
Current configuration : 3464 bytes
!
version 15.9
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname AS01-P04
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
mpls traffic-eng tunnels
!
!
!
!
!
redundancy
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 172.17.0.4 255.255.255.255
!
interface GigabitEthernet0/0
 ip address 172.16.2.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls traffic-eng tunnels
 mpls ip
 ip rsvp bandwidth
!
interface GigabitEthernet0/1
 ip address 172.16.1.2 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls traffic-eng tunnels
 mpls ip
 ip rsvp bandwidth
!
interface GigabitEthernet0/2
 ip address 172.16.30.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls traffic-eng tunnels
 mpls ip
 ip rsvp bandwidth
!
interface GigabitEthernet0/3
 ip address 172.16.40.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls traffic-eng tunnels
 mpls ip
 ip rsvp bandwidth
!
router ospf 1
 mpls traffic-eng router-id Loopback0
 mpls traffic-eng area 0
 network 172.16.0.0 0.0.255.255 area 0
 network 172.17.0.0 0.0.0.255 area 0
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 ioam timestamp
!
!
!
control-plane
!
banner exec <
>
!
line con 0
 exec-timeout 0 0
line aux 0
line vty 0 4
 exec-timeout 0 0
 login
 transport input none
!
no scheduler allocate
!
end

##################################################################################

AS01-PE01
Current configuration : 7363 bytes
!
! Last configuration change at 07:37:26 UTC Tue Aug 27 2024
!
version 17.3
service timestamps debug datetime msec
service timestamps log datetime msec
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
platform console serial
!
hostname AS01-PE01
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
!
!
!
!
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
! 
! 
! 
! 
!
!
mpls ldp label
 allocate global host-routes
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
crypto pki trustpoint TP-self-signed-4270505333
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-4270505333
 revocation-check none
 rsakeypair TP-self-signed-4270505333
!
!
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030 
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363 
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934 
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305 
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720 
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030 
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D 
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520 
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE 
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC 
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188 
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7 
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191 
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44 
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201 
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85 
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500 
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905 
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B 
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8 
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C 
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B 
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678 
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB 
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0 
  D697DF7F 28
  quit
crypto pki certificate chain TP-self-signed-4270505333
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030 
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274 
  69666963 6174652D 34323730 35303533 3333301E 170D3233 30363133 31343138 
  31355A17 0D333330 36313231 34313831 355A3031 312F302D 06035504 03132649 
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D34 32373035 
  30353333 33308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201 
  0A028201 0100A053 B57CFCCF 3E0D932A EC175225 4D35EDB5 12C6C7CB E1A041A4 
  DAD45D68 5E8CC1B6 EEE0F8A7 822256F8 EFAFE581 8B34F842 94DD9D7E 2A260B4B 
  1CA57D21 D9A77EAB 1131B923 A30DFE7E 2BA71561 D098C70A F2B2AEC3 33E448D4 
  42F9FF9E 52A6A387 70459986 08F89C8F E1806D15 81423497 9A4F3D5F 6FF7FF46 
  BB825C76 9A703AF5 663BCD98 074775AB EF964DC4 547E6D19 C70389EA 0299D298 
  27499768 B2D1245E 281E3B74 963123B0 7A0A56B0 343D7A71 EA47DD9B A20EE451 
  3B3AC7A1 0D1E227B 257F9A50 21869198 B85AB4EE 3C9640D9 CD3E053C 6C5A6307 
  F3BE8A49 D3DCA7B3 5D5B2D3F A6056343 2D521121 5EA67216 61392C05 A266AB20 
  F5A50BC2 3E730203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF 
  301F0603 551D2304 18301680 148DEFD3 BA2D5FEE 186D18D2 5E416553 02B3FD17 
  0D301D06 03551D0E 04160414 8DEFD3BA 2D5FEE18 6D18D25E 41655302 B3FD170D 
  300D0609 2A864886 F70D0101 05050003 82010100 31F3C2C6 CEB1E0BB C57D6FC2 
  288B56FE F475F44C E1A41C7E 88942D17 CC6B4EA8 F55859FA B2338EFE 19BB113A 
  B5D0C27B C3D3274E D63A08EB 6BA67D8A E784C7ED 5F8C0CD0 37D4E23F 472EA4A8 
  DB6800C2 12B0B9FB FA0FA61E EB575EDB 4A753254 A8544C44 9AF08427 AA1E074B 
  409CE4E9 72557F85 FC5ACB0B 9A093F5F C94B0360 87533145 646A887E 6EF925BA 
  346D0D30 95684F8A FDF2AADD C4519C70 6C8062DB 7694D8E8 8351803F 7B5FD21A 
  DDFF4E57 F8D43EF7 5CA72CD9 570079B3 668E7525 25BA9103 49DC8F75 0C5F8F84 
  84351DE8 B2A067A2 6B7BDD49 3623BE0A B377B62C B0C1CD72 543CEC98 18C7B0F9 
  8BFC2040 ACC6E8E1 C34D70BE E783B6ED F09FB9FB
  quit
!
license udi pid CSR1000V sn 9SWGZ8AE708
diagnostic bootup level minimal
memory free low-watermark processor 71489
!
!
spanning-tree extend system-id
!
!
redundancy
!
bridge-domain 21 
 no mac learning
!
!
!
!
!
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
!
! 
! 
!
!
interface Loopback0
 ip address 172.17.0.10 255.255.255.255
!
interface GigabitEthernet1
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 121 ethernet
  encapsulation dot1q 121
  rewrite ingress tag pop 1 symmetric
  bridge-domain 21
 !
!
interface GigabitEthernet2
 ip address 172.16.10.2 255.255.255.0
 negotiation auto
 mpls ip
 no mop enabled
 no mop sysid
!
interface GigabitEthernet3
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 122 ethernet
  encapsulation dot1q 122
  rewrite ingress tag pop 1 symmetric
  bridge-domain 21
 !
!
interface GigabitEthernet4
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 131 ethernet
  encapsulation dot1q 131
  rewrite ingress tag pop 1 symmetric
  xconnect 172.17.0.30 31 encapsulation mpls
 !
!
interface GigabitEthernet5
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 141 ethernet
  encapsulation dot1q 141
  rewrite ingress tag pop 1 symmetric
  xconnect 172.17.0.50 41 encapsulation mpls
   backup peer 172.17.0.60 51
 !
!
interface GigabitEthernet6
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 1121 ethernet
  encapsulation dot1q 1121
  rewrite ingress tag pop 1 symmetric
 !
!
interface GigabitEthernet7
 no ip address
 shutdown
 negotiation auto
 no mop enabled
 no mop sysid
!
interface GigabitEthernet8
 no ip address
 shutdown
 negotiation auto
 no mop enabled
 no mop sysid
!
router ospf 1
 network 172.16.0.0 0.0.255.255 area 0
 network 172.17.0.0 0.0.0.255 area 0
!
ip forward-protocol nd
no ip http server
ip http secure-server
!
!
!
!
!
!
!
!
control-plane
!
!
!
!
!
!
line con 0
 exec-timeout 0 0
 stopbits 1
line vty 0
 exec-timeout 0 0
 login
 transport input ssh
line vty 1
 exec-timeout 0 0
 login
 length 0
 transport input ssh
line vty 2 4
 exec-timeout 0 0
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
end

##################################################################################

AS01-PE02
Current configuration : 7921 bytes
!
! Last configuration change at 14:32:20 UTC Tue Aug 27 2024
!
version 17.3
service timestamps debug datetime msec
service timestamps log datetime msec
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
platform console serial
!
hostname AS01-PE02
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
!
!
!
!
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
! 
! 
! 
! 
!
!
mpls ldp label
 allocate global host-routes
multilink bundle-name authenticated
l2vpn vfi context LAB006 
 vpn id 61
 member 172.17.0.60 encapsulation mpls
 member 172.17.0.50 encapsulation mpls
 member 172.17.0.30 encapsulation mpls
!
l2vpn vfi context LAB007 
 vpn id 71
 autodiscovery bgp signaling ldp 
  rd 1:71
  route-target export 1:71
  route-target import 1:71
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
crypto pki trustpoint TP-self-signed-2752672816
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-2752672816
 revocation-check none
 rsakeypair TP-self-signed-2752672816
!
!
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030 
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363 
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934 
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305 
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720 
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030 
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D 
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520 
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE 
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC 
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188 
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7 
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191 
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44 
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201 
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85 
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500 
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905 
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B 
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8 
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C 
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B 
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678 
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB 
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0 
  D697DF7F 28
  quit
crypto pki certificate chain TP-self-signed-2752672816
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030 
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274 
  69666963 6174652D 32373532 36373238 3136301E 170D3233 30363133 31343138 
  30305A17 0D333330 36313231 34313830 305A3031 312F302D 06035504 03132649 
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D32 37353236 
  37323831 36308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201 
  0A028201 0100B54F 512F3FFB 7FA18C6B D2405A26 6CC52807 AA405419 D69BD9BD 
  FBACF507 129A8ED7 D4C57593 EB4693D3 4E085D88 CCB051A3 9B795F5E EE47EA87 
  3D4312CF 5D662050 F838DF09 26BBEB07 2F3603B7 2FA3904D B8C898E4 9B359056 
  282C2EE2 62B1962A 7AAF5131 20D89849 10B6891D 7694C8F6 9175CF88 84A0A75C 
  D0F4EFD0 8740B567 3FE6D7BE 6FE9C2E3 3ACE07EF 02DB5853 0D4BA50D DA74C928 
  11D65797 423668BB F76D75DD 3B0D4D8A 5C8AADB5 9866C0FA 21CABC08 AF33D42B 
  F4C599A9 A6AC4C28 F694113B 55050D13 B9C45587 6057F3F4 8BC9B6D3 106431F8 
  9C175D9C D2B0F006 6161A8CF A9654A82 0CBBB689 CDFD0B09 F10BB7C3 E68D02D0 
  30B5F225 927B0203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF 
  301F0603 551D2304 18301680 147AE9AE A8C81E0D AF47B818 63E5AAF2 4B615B05 
  B2301D06 03551D0E 04160414 7AE9AEA8 C81E0DAF 47B81863 E5AAF24B 615B05B2 
  300D0609 2A864886 F70D0101 05050003 82010100 5B7A35B2 7160C63C 5CD14C82 
  51220666 5F352E91 9BD2A450 D723621C 433DF6D5 F94ADDD7 01A59E4D 4D6B330E 
  C2725AB1 1630775C 5F56F873 7B0423C7 EC997E46 022ED078 2F96C686 45A82A09 
  45BF6ACA B6F94C79 C2B2C355 CDEEB5B6 D93697BF DF9281DE C1AD1A42 9F0B801F 
  FDD6D106 2D17F19E 4252771E 05201419 914DE276 6B0E01D0 4E9F4958 F39097D5 
  34953EC9 9F54422A C8E156FC F5B06A04 44FA4971 8E1E430F DA7F4592 F4764E03 
  02F96262 C862FDB3 58F3D83B 2AC0E0A2 AE8D0DEC 884D96C0 30207E90 5A5D9A24 
  BE0E277F 5C4F6B93 1AF08333 F383C7A0 D8CA6012 882F508F 6BD543DC 352BF494 
  76062578 71F57B46 10228C4C FF71EE0F 4E43284C
  quit
!
license udi pid CSR1000V sn 93RA0YBFF5M
diagnostic bootup level minimal
memory free low-watermark processor 71489
!
!
spanning-tree extend system-id
!
!
redundancy
!
bridge-domain 61 
 member GigabitEthernet4 service-instance 261
 member vfi LAB006
!
bridge-domain 71 
 member GigabitEthernet5 service-instance 271
 member vfi LAB007
!
!
!
!
!
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
!
! 
! 
!
!
interface Loopback0
 ip address 172.17.0.20 255.255.255.255
!
interface pseudowire32
 encapsulation mpls
 neighbor 172.17.0.40 32
!
interface pseudowire41
 encapsulation mpls
 neighbor 172.17.0.50 41
!
interface pseudowire51
 encapsulation mpls
 neighbor 172.17.0.60 51
!
interface GigabitEthernet1
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 231 ethernet
  encapsulation dot1q 231
  rewrite ingress tag pop 1 symmetric
 !
!
interface GigabitEthernet2
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 241 ethernet
  encapsulation dot1q 241
  rewrite ingress tag pop 1 symmetric
 !
!
interface GigabitEthernet3
 ip address 172.16.20.2 255.255.255.0
 negotiation auto
 mpls ip
 no mop enabled
 no mop sysid
!
interface GigabitEthernet4
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 261 ethernet
  encapsulation dot1q 261
  rewrite ingress tag pop 1 symmetric
 !
!
interface GigabitEthernet5
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 271 ethernet
  encapsulation dot1q 271
  rewrite ingress tag pop 1 symmetric
 !
!
router ospf 1
 network 172.16.0.0 0.0.255.255 area 0
 network 172.17.0.0 0.0.0.255 area 0
!
router bgp 1
 bgp log-neighbor-changes
 neighbor 172.17.0.100 remote-as 1
 neighbor 172.17.0.100 update-source Loopback0
 !
 address-family l2vpn vpls
  neighbor 172.17.0.100 activate
 exit-address-family
!
ip forward-protocol nd
no ip http server
ip http secure-server
!
!
!
!
!
l2vpn xconnect context LAB003
 member pseudowire32
 member GigabitEthernet1 service-instance 231 
!
l2vpn xconnect context LAB004
 member pseudowire41 group LAB005 priority 1
 member pseudowire51 group LAB005 priority 2
 member GigabitEthernet2 service-instance 241 
!
!
!
!
control-plane
!
!
!
!
!
!
line con 0
 exec-timeout 0 0
 stopbits 1
line vty 0
 exec-timeout 0 0
 login
 transport input ssh
line vty 1
 exec-timeout 0 0
 login
 length 0
 transport input ssh
line vty 2 4
 exec-timeout 0 0
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
end

##################################################################################

AS01-PE03
Current configuration : 7407 bytes
!
! Last configuration change at 14:34:43 UTC Tue Aug 27 2024
!
version 17.3
service timestamps debug datetime msec
service timestamps log datetime msec
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
platform console serial
!
hostname AS01-PE03
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
!
!
!
!
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
! 
! 
! 
! 
!
!
mpls ldp label
 allocate global host-routes
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
crypto pki trustpoint TP-self-signed-2623508560
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-2623508560
 revocation-check none
 rsakeypair TP-self-signed-2623508560
!
!
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030 
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363 
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934 
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305 
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720 
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030 
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D 
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520 
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE 
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC 
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188 
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7 
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191 
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44 
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201 
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85 
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500 
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905 
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B 
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8 
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C 
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B 
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678 
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB 
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0 
  D697DF7F 28
  quit
crypto pki certificate chain TP-self-signed-2623508560
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030 
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274 
  69666963 6174652D 32363233 35303835 3630301E 170D3233 30363133 31343138 
  32335A17 0D333330 36313231 34313832 335A3031 312F302D 06035504 03132649 
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D32 36323335 
  30383536 30308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201 
  0A028201 0100C9D1 86695F27 A7A96388 F0127EAE BFF955BD 4AC708D4 E9C391F2 
  C45979A4 C641FB4E C8A1D2C9 4868AB33 BCB4ADF5 69276DA9 E209E8B7 06A8AF32 
  29227278 7D06FAB3 42A0133E 31F2D816 E0EDEB7D E8E0A0D5 67F2D4B4 0C46B6B7 
  91C0F225 EE887F0E D5F566AB 51A014C2 F37EBB5E 90298199 E477B443 DE69B683 
  5CADFC6E 9EDC492F E90C1B64 987910CC 953A2EB1 FFAAC57D EEE796B1 E1C6C2AE 
  EF4A56B5 D1AF0016 8F3E3F3C 323E7D18 F7B67ABC 54771662 FE9E87C6 20F0A0CF 
  9DF0EABF 8C833EF9 A4F85186 CF5A16FB 0C3E59C1 5174FFD3 0EF6C27B 69F517AD 
  9F141993 5EE4B2CA 5C630DFE 6E5EB443 C2867754 2010F4FF 07899885 7D78E18D 
  1E12965D 77E70203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF 
  301F0603 551D2304 18301680 14FDAD69 60FC5DFD 586448F3 A290EBF2 477A6183 
  3A301D06 03551D0E 04160414 FDAD6960 FC5DFD58 6448F3A2 90EBF247 7A61833A 
  300D0609 2A864886 F70D0101 05050003 82010100 28F5A183 D20C6ED4 6B95256A 
  102E3391 02D3FED0 65B67D7E AF936E7A 5FE7FE55 B0FAD385 513D6695 0A7500C0 
  F72AFEE4 BA646BC0 205954C3 6F0A9211 F56E4C32 F80A1BA9 33389403 504E8384 
  76C97217 8FF9CE63 CDE875A3 15504E00 84D30036 C2950B88 83B71411 52A24C7B 
  171247BF 5CFFA90B 491E7DF8 84DC9130 2FD11041 1545A1AD 15C6467D 353FF00A 
  A6CA74D3 25D4AB0B 951BCB08 B37A20E7 420CAE01 E5AF59A7 B85B3F17 8D52E3C1 
  0688119F 7E315A16 DC44982C 15EDFDA8 E2D1F2CA D4EF3B17 89CAF827 FC70B9F7 
  A4C19805 9FEAED0D D17F5B7C 5EDFC43B FB8C26A7 F231138B 12C501F4 6CEB31E7 
  56F38261 0D930009 7210102C 38FDEA1F 7ED53673
  quit
!
license udi pid CSR1000V sn 9VQS6ZNSMVG
diagnostic bootup level minimal
memory free low-watermark processor 71489
!
!
spanning-tree extend system-id
!
!
redundancy
!
!
!
!
!
!
!
l2 vfi LAB006 manual 
 vpn id 61
 bridge-domain 61
 neighbor 172.17.0.60 encapsulation mpls
 neighbor 172.17.0.50 encapsulation mpls
 neighbor 172.17.0.20 encapsulation mpls
!
l2 vfi LAB007 autodiscovery 
 vpn id 71
 bridge-domain 71
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
!
! 
! 
!
!
interface Loopback0
 ip address 172.17.0.30 255.255.255.255
!
interface GigabitEthernet1
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 131 ethernet
 !
 service instance 331 ethernet
  encapsulation dot1q 331
  rewrite ingress tag pop 1 symmetric
  xconnect 172.17.0.10 31 encapsulation mpls
 !
!
interface GigabitEthernet2
 ip address 172.16.30.2 255.255.255.0
 negotiation auto
 mpls ip
 no mop enabled
 no mop sysid
!
interface GigabitEthernet3
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 341 ethernet
  encapsulation dot1q 341
  rewrite ingress tag pop 1 symmetric
  xconnect 172.17.0.50 41 encapsulation mpls
   backup peer 172.17.0.60 51
 !
!
interface GigabitEthernet4
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 361 ethernet
  encapsulation dot1q 361
  rewrite ingress tag pop 1 symmetric
  bridge-domain 61
 !
!
interface GigabitEthernet5
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 371 ethernet
  encapsulation dot1q 371
  rewrite ingress tag pop 1 symmetric
  bridge-domain 71
 !
!
router ospf 1
 network 172.16.0.0 0.0.255.255 area 0
 network 172.17.0.0 0.0.0.255 area 0
!
router bgp 1
 bgp log-neighbor-changes
 neighbor 172.17.0.100 remote-as 1
 neighbor 172.17.0.100 update-source Loopback0
 !
 address-family l2vpn vpls
  neighbor 172.17.0.100 activate
 exit-address-family
!
ip forward-protocol nd
no ip http server
ip http secure-server
!
!
!
!
!
!
!
!
control-plane
!
!
!
!
!
!
line con 0
 exec-timeout 0 0
 stopbits 1
line vty 0
 exec-timeout 0 0
 login
 transport input ssh
line vty 1
 exec-timeout 0 0
 login
 length 0
 transport input ssh
line vty 2 4
 exec-timeout 0 0
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
end

##################################################################################

AS01-PE04 (XR) 
Wed Aug 28 09:11:18.534 UTCRP/0/RP0/CPU0:AS01-PE04#show run
Wed Aug 28 09:11:20.899 UTCBuilding configuration...!! IOS XR Configuration 7.7.1!! Last configuration change at Tue Aug 27 14:43:51 2024 by cisco!hostname AS01-PE04logging console disableusername cisco group root-lr group cisco-support password 7 01100F175804!username admin group root-lr group cisco-support password 7 011202095205!username lab group root-lr group cisco-support password 7 12150415!line console exec-timeout 0 0 absolute-timeout 0 session-timeout 0!line default exec-timeout 0 0 absolute-timeout 0 session-timeout 0!call-home service active contact smart-licensing profile CiscoTAC-1  active  destination transport-method email disable  destination transport-method http !!interface Loopback0 ipv4 address 172.17.0.40 255.255.255.255!interface MgmtEth0/RP0/CPU0/0 shutdown!interface GigabitEthernet0/0/0/0.422 l2transport encapsulation dot1q 422 rewrite ingress tag pop 1 symmetric!interface GigabitEthernet0/0/0/1.421 l2transport encapsulation dot1q 421 rewrite ingress tag pop 1 symmetric!interface GigabitEthernet0/0/0/2.431 l2transport encapsulation dot1q 431 rewrite ingress tag pop 1 symmetric!interface GigabitEthernet0/0/0/3 ipv4 address 172.16.40.2 255.255.255.0!interface GigabitEthernet0/0/0/4.441 l2transport encapsulation dot1q 441 rewrite ingress tag pop 1 symmetric!interface GigabitEthernet0/0/0/5.481 l2transport encapsulation dot1q 481 rewrite ingress tag pop 1 symmetric!interface GigabitEthernet0/0/0/6.4121 l2transport encapsulation dot1q 412 rewrite ingress tag pop 1 symmetric!interface GigabitEthernet0/0/0/7 shutdown!router ospf 1 area 0  interface Loopback0   passive enable  !  interface GigabitEthernet0/0/0/3  ! !!l2vpn xconnect group LAB003  p2p LAB003   interface GigabitEthernet0/0/0/2.431   neighbor ipv4 172.17.0.20 pw-id 32   !  ! ! xconnect group LAB004  p2p LAB004   interface GigabitEthernet0/0/0/4.441   neighbor ipv4 172.17.0.50 pw-id 41    backup neighbor 172.17.0.60 pw-id 51    !   !  ! ! xconnect group LAB008  p2p LAB008   interface GigabitEthernet0/0/0/5.481   neighbor ipv4 172.17.0.200 pw-id 82   !  ! !!mpls ldp address-family ipv4  label   local    allocate for host-routes   !  ! ! interface GigabitEthernet0/0/0/3 !!end
RP/0/RP0/CPU0:AS01-PE04#

##################################################################################

AS01-PE05
Current configuration : 8284 bytes
!
! Last configuration change at 08:25:21 UTC Wed Aug 28 2024
!
version 17.3
service timestamps debug datetime msec
service timestamps log datetime msec
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
platform console serial
!
hostname AS01-PE05
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
!
!
!
!
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
! 
! 
! 
! 
!
!
mpls ldp label
 allocate global host-routes
mpls ldp discovery targeted-hello accept
multilink bundle-name authenticated
l2vpn vfi context LAB006 
 vpn id 61
 member 172.17.0.60 encapsulation mpls
 member 172.17.0.30 encapsulation mpls
 member 172.17.0.20 encapsulation mpls
!
l2vpn vfi context LAB007 
 vpn id 71
 autodiscovery bgp signaling ldp 
  rd 1:71
  route-target export 1:71
  route-target import 1:71
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
crypto pki trustpoint TP-self-signed-759245963
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-759245963
 revocation-check none
 rsakeypair TP-self-signed-759245963
!
!
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030 
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363 
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934 
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305 
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720 
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030 
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D 
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520 
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE 
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC 
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188 
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7 
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191 
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44 
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201 
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85 
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500 
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905 
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B 
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8 
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C 
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B 
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678 
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB 
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0 
  D697DF7F 28
  quit
crypto pki certificate chain TP-self-signed-759245963
 certificate self-signed 01
  3082032E 30820216 A0030201 02020101 300D0609 2A864886 F70D0101 05050030 
  30312E30 2C060355 04031325 494F532D 53656C66 2D536967 6E65642D 43657274 
  69666963 6174652D 37353932 34353936 33301E17 0D323330 36313331 34313734 
  395A170D 33333036 31323134 31373439 5A303031 2E302C06 03550403 1325494F 
  532D5365 6C662D53 69676E65 642D4365 72746966 69636174 652D3735 39323435 
  39363330 82012230 0D06092A 864886F7 0D010101 05000382 010F0030 82010A02 
  82010100 D19E6C5D DD91C401 097322E7 AC81E507 DF5EB864 ED01DA09 A2F7E2E9 
  D547618B 4F732A04 2261E637 E2D78509 D5C609E7 6462AB7F 340A7D61 E88A5720 
  CE92F342 9C482618 E4AA77B0 2A00615D 243DD01F 8C5594E6 2FDA3B0A FC65B285 
  F9BAE10C 3DEBFBDD 84BB8B20 BA2D0E7F A78ABFFD B20F2970 42A55AE1 0A37F7C5 
  38B0F60F 14D290DA B2D9BFDE 7B1EC2C2 0101EC01 90076AB3 04E4CFE5 CD1B9B49 
  55F87F98 39E5E4CA 1282FBD3 B45F77E0 1F0DEE68 DB3AAED2 F41AF47C FD486575 
  AC6A5591 6EBDEB43 D9323E9B EE4CDE7D CDF6978B B0955790 AC834121 F23D846A 
  36AF3B2E 72DD8766 B0776FEB B35513BD 91F5DA0D 9DB20E88 C6B7B1E7 05BC9DE2 
  8DB19F47 02030100 01A35330 51300F06 03551D13 0101FF04 05300301 01FF301F 
  0603551D 23041830 168014D4 790FEC5B 28E31BE9 4DB078A0 B5FE7F54 11FC2730 
  1D060355 1D0E0416 0414D479 0FEC5B28 E31BE94D B078A0B5 FE7F5411 FC27300D 
  06092A86 4886F70D 01010505 00038201 0100624A F865C170 99DB16EA 348C2374 
  93AD38D1 85D5509B 27CAA404 FF3B55D9 54286DC4 F58F940A 8D065C0E AAA7A257 
  2D3F011A B5ACD484 DC1D0570 3916257D 6DDC47A3 B80DB5B8 8A47B9F8 9AD2B6AF 
  EC1512B3 F5EAA1AF C8AB4C4F B906E415 A79670DA 098B84D6 5E719641 A031B5D6 
  804933E7 4B83066E FC1560B2 2EC6D186 0601CF8B AF5FFF45 16621486 47B14BB2 
  FECBDE10 4289D4B6 F0E0F15C D83F9D46 8E1AFEC9 3E41DBE8 3215A8DB EBF265CF 
  D7357756 F3D5326B C9B7AD7F A4741D20 A845AA45 E40DC9C7 2388700D 829045FD 
  5A41ADDF 3B038887 74E9FF35 BC9F5AB2 28B27DEC 38BF8B1D 4EAC3202 C3D889D9 
  A100CB75 C9CB9CD4 0ACAA0E6 3CBBDD72 CE4A
  quit
!
license udi pid CSR1000V sn 9KVA7BHRNMH
diagnostic bootup level minimal
memory free low-watermark processor 71489
!
!
spanning-tree extend system-id
!
!
redundancy
!
bridge-domain 61 
 member GigabitEthernet1 service-instance 561
 member vfi LAB006
!
bridge-domain 71 
 member GigabitEthernet3 service-instance 571
 member vfi LAB007
!
!
!
!
!
!
!
l2 pseudowire routing
 terminating-pe tie-breaker
l2 vfi LAB004 manual 
 vpn id 41
 bridge-domain 41
 neighbor 172.17.0.10 encapsulation mpls no-split-horizon
 neighbor 172.17.0.20 encapsulation mpls no-split-horizon
 neighbor 172.17.0.30 encapsulation mpls no-split-horizon
 neighbor 172.17.0.40 encapsulation mpls no-split-horizon
!
l2 vfi LAB010 autodiscovery 
 vpn id 101
 bridge-domain 101
 vpls-id 10:1
 rd 10:1
 route-target export 10:1
 route-target import 10:1
 no auto-route-target
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
!
! 
! 
!
!
interface Loopback0
 ip address 172.17.0.50 255.255.255.255
!
interface GigabitEthernet1
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 561 ethernet
  encapsulation dot1q 561
  rewrite ingress tag pop 1 symmetric
 !
!
interface GigabitEthernet2
 ip address 172.16.50.2 255.255.255.0
 negotiation auto
 mpls ip
 no mop enabled
 no mop sysid
!
interface GigabitEthernet3
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 571 ethernet
  encapsulation dot1q 571
  rewrite ingress tag pop 1 symmetric
 !
!
interface GigabitEthernet4
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 581 ethernet
  encapsulation dot1q 581
  rewrite ingress tag pop 1 symmetric
  xconnect 172.17.0.200 81 encapsulation mpls
 !
!
interface GigabitEthernet5
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 511 ethernet
  encapsulation dot1q 511
  rewrite ingress tag pop 1 symmetric
  bridge-domain 101
 !
!
interface GigabitEthernet6
 no ip address
 negotiation auto
 no keepalive
 no mop enabled
 no mop sysid
 service instance 5121 ethernet
  encapsulation dot1q 512
  rewrite ingress tag pop 1 symmetric
 !
!
router ospf 1
 network 172.16.0.0 0.0.255.255 area 0
 network 172.17.0.0 0.0.0.255 area 0
!
router bgp 1
 bgp log-neighbor-changes
 neighbor 172.17.0.100 remote-as 1
 neighbor 172.17.0.100 update-source Loopback0
 !
 address-family l2vpn vpls
  neighbor 172.17.0.100 activate
  neighbor 172.17.0.100 send-community both
 exit-address-family
!
ip forward-protocol nd
no ip http server
ip http secure-server
!
!
!
!
!
!
!
!
control-plane
!
!
!
!
!
!
line con 0
 exec-timeout 0 0
 stopbits 1
line vty 0
 exec-timeout 0 0
 login
 transport input ssh
line vty 1
 exec-timeout 0 0
 login
 length 0
 transport input ssh
line vty 2 4
 exec-timeout 0 0
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
end

##################################################################################

AS01-PE06
Current configuration : 8200 bytes
!
! Last configuration change at 07:37:19 UTC Wed Aug 28 2024
!
version 17.3
service timestamps debug datetime msec
service timestamps log datetime msec
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
platform console serial
!
hostname AS01-PE06
!
boot-start-marker
boot-end-marker
!
!
vrf definition LAB009
 rd 9:1
 !
 address-family ipv4
  route-target export 9:1
  route-target import 9:1
 exit-address-family
!
no logging console
!
no aaa new-model
!
!
!
!
!
!
!
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
! 
! 
! 
! 
!
!
mpls ldp label
 allocate global host-routes
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
crypto pki trustpoint TP-self-signed-1796693582
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-1796693582
 revocation-check none
 rsakeypair TP-self-signed-1796693582
!
!
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030 
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363 
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934 
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305 
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720 
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030 
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D 
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520 
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE 
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC 
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188 
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7 
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191 
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44 
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201 
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85 
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500 
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905 
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B 
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8 
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C 
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B 
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678 
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB 
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0 
  D697DF7F 28
  quit
crypto pki certificate chain TP-self-signed-1796693582
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030 
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274 
  69666963 6174652D 31373936 36393335 3832301E 170D3233 30363133 31343138 
  32335A17 0D333330 36313231 34313832 335A3031 312F302D 06035504 03132649 
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 37393636 
  39333538 32308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201 
  0A028201 01009ADD 36D84DF0 EDDFC062 87CB0CBA CD54B35F 9FE1FA46 802CB53B 
  EE107C5D AE4E4000 D7BE3DC1 DE102820 CF1185C9 5F3AFAD4 F5DBFB32 ECAB2987 
  EA3570BD 038C7117 4621A448 73CB68DC DFCAE39A 578AE7B3 E0A8D1A3 DFB8BFDB 
  2AEA61F0 022B2F7A 6E2EFCDA 5B40B94E 0150E56D CE78FE0A 976F8A4E 1F92C9C4 
  AD39B39E AD1E80CC 1ABF1078 C561C121 BC31CEC3 363024F5 54F69528 74D2F9BB 
  1D08E94A 2842D1C7 15AB91D4 B0C962BD 19EED915 D073C475 4BAED474 E0D70D1F 
  ED31AD3A C637E8F3 6CDB187F 5B48A2A6 13C6B106 BE0D7B24 07B17BB7 EE9CD65F 
  6CDDB5CD 748D8E86 DEEFE44B 00FC5F6A F8D086F1 C60605A3 A57555D2 483A100C 
  0CF620F6 EAF50203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF 
  301F0603 551D2304 18301680 14413B02 11AC51BC 72A1BF5B E63AFC92 2D950D7D 
  AF301D06 03551D0E 04160414 413B0211 AC51BC72 A1BF5BE6 3AFC922D 950D7DAF 
  300D0609 2A864886 F70D0101 05050003 82010100 10D94ACC A01E9D8C 37CDB3C2 
  E7BF4565 150FD18C 325807B2 99E2B828 04DC9B70 4B93031F 694A511F 087314EC 
  5F7C6924 0FEB8F52 5EC408F8 761BAF64 9C98B6EC E0B828B0 AE919B00 7B440AB0 
  C31FDB05 DBF0CB69 6A4F120D 13DCCCAB 506C9A89 715DD838 47F09BDB 405515A7 
  CA3618EC 16B55FE4 37DD597D 78FF1D3C E95F4027 1C4F95F0 D9838DB0 DF9A0045 
  CE8CEC3A D454B61D 6272014A 3D3F4932 DFE90C2A 7F1B84B6 34DDED8E 68E1B2D0 
  8F039ECA C5AFBCA6 EFFF5E6A 0E8F049B C98C3D48 27E453BC 0F7AC128 381CBE23 
  3A394CC5 76C6F318 E0224DF5 89634CF4 852AA42C 60EFE34B 9D7D2751 ADBE6899 
  AA2A08CA 483116C8 9D4CD458 F22EAAE9 D7E28375
  quit
!
license udi pid CSR1000V sn 95XK3JK00ST
diagnostic bootup level minimal
memory free low-watermark processor 71489
!
!
spanning-tree extend system-id
!
!
redundancy
!
!
!
!
!
!
!
l2 vfi LAB005 manual 
 vpn id 51
 bridge-domain 51
 neighbor 172.17.0.10 encapsulation mpls no-split-horizon
 neighbor 172.17.0.20 encapsulation mpls no-split-horizon
 neighbor 172.17.0.30 encapsulation mpls no-split-horizon
 neighbor 172.17.0.40 encapsulation mpls no-split-horizon
!
l2 vfi LAB006 manual 
 vpn id 61
 bridge-domain 61
 neighbor 172.17.0.50 encapsulation mpls
 neighbor 172.17.0.30 encapsulation mpls
 neighbor 172.17.0.20 encapsulation mpls
!
l2 vfi LAB007 autodiscovery 
 vpn id 71
 bridge-domain 71
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
!
! 
! 
!
!
interface Loopback0
 ip address 172.17.0.60 255.255.255.255
!
interface GigabitEthernet1
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 661 ethernet
  encapsulation dot1q 661
  rewrite ingress tag pop 1 symmetric
  bridge-domain 61
 !
!
interface GigabitEthernet2
 ip address 172.16.60.2 255.255.255.0
 negotiation auto
 mpls ip
 no mop enabled
 no mop sysid
!
interface GigabitEthernet3
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 671 ethernet
  encapsulation dot1q 671
  rewrite ingress tag pop 1 symmetric
  bridge-domain 71
 !
!
interface GigabitEthernet4
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 691 ethernet
  encapsulation dot1q 691
  rewrite ingress tag pop 1 symmetric
  bridge-domain 91
 !
!
interface GigabitEthernet5
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 611 ethernet
  encapsulation dot1q 611
  rewrite ingress tag pop 1 symmetric
 !
!
interface GigabitEthernet6
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 6121 ethernet
  encapsulation dot1q 621
  rewrite ingress tag pop 1 symmetric
 !
!
interface BDI91
 vrf forwarding LAB009
 ip address 10.6.9.2 255.255.255.0
 no mop enabled
 no mop sysid
!
router ospf 1
 network 172.16.0.0 0.0.255.255 area 0
 network 172.17.0.0 0.0.0.255 area 0
!
router bgp 1
 bgp log-neighbor-changes
 neighbor 172.17.0.100 remote-as 1
 neighbor 172.17.0.100 update-source Loopback0
 !
 address-family vpnv4
  neighbor 172.17.0.100 activate
  neighbor 172.17.0.100 send-community both
 exit-address-family
 !
 address-family l2vpn vpls
  neighbor 172.17.0.100 activate
 exit-address-family
 !
 address-family ipv4 vrf LAB009
  network 10.6.9.0 mask 255.255.255.0
 exit-address-family
!
ip forward-protocol nd
no ip http server
ip http secure-server
!
!
!
!
!
!
!
!
control-plane
!
!
!
!
!
!
line con 0
 exec-timeout 0 0
 stopbits 1
line vty 0
 exec-timeout 0 0
 login
 transport input ssh
line vty 1
 exec-timeout 0 0
 login
 length 0
 transport input ssh
line vty 2 4
 exec-timeout 0 0
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
end

##################################################################################

AS01-RR01
Current configuration : 7159 bytes
!
! Last configuration change at 08:25:56 UTC Wed Aug 28 2024
!
version 17.3
service timestamps debug datetime msec
service timestamps log datetime msec
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
platform console serial
!
hostname AS01-RR01
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
!
!
!
!
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
! 
! 
! 
! 
!
!
mpls ldp label
 allocate global host-routes
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
crypto pki trustpoint TP-self-signed-321543689
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-321543689
 revocation-check none
 rsakeypair TP-self-signed-321543689
!
!
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030 
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363 
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934 
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305 
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720 
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030 
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D 
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520 
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE 
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC 
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188 
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7 
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191 
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44 
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201 
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85 
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500 
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905 
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B 
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8 
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C 
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B 
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678 
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB 
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0 
  D697DF7F 28
  quit
crypto pki certificate chain TP-self-signed-321543689
 certificate self-signed 01
  3082032E 30820216 A0030201 02020101 300D0609 2A864886 F70D0101 05050030 
  30312E30 2C060355 04031325 494F532D 53656C66 2D536967 6E65642D 43657274 
  69666963 6174652D 33323135 34333638 39301E17 0D323330 36313331 34313830 
  345A170D 33333036 31323134 31383034 5A303031 2E302C06 03550403 1325494F 
  532D5365 6C662D53 69676E65 642D4365 72746966 69636174 652D3332 31353433 
  36383930 82012230 0D06092A 864886F7 0D010101 05000382 010F0030 82010A02 
  82010100 ABC7DDA6 0E0DBE59 649658D4 CDB4540D 9AA995CD 07A9CDD5 3DCECD9C 
  2AD9F4F3 9A2289FA 6CE2F9FB A0697967 9C660B8E 0DE7F635 570582CA A306A651 
  C7F4BDFC 36191722 57DE7E6A 941E73E5 721FD0A0 0388D0CA 59B19334 FC65B052 
  EDDCF08A 7F4EC359 45374396 E0A5D109 40AE551E F2DD1862 20B242A1 26B29B71 
  9BDF3E9B D7278CDD DBA844A2 0E9AC8BA 7DF236B3 0B48C402 34C03D04 CE56DA29 
  1602ACAF C371B17E 1C86B831 F11AD72C A9614727 A4179083 568F9EBB C22033E0 
  987C60CD A0E70F04 DE499780 08E7C971 F2DFB8DE 9444EF1E 99C8C4CF C7FF5CF9 
  FD5453DF D784DA29 8342787D 86B92764 4D6699BF 6F319CDA 346F9B7C 9A6B7294 
  DC7D1AD5 02030100 01A35330 51300F06 03551D13 0101FF04 05300301 01FF301F 
  0603551D 23041830 168014FE 3796B96F FADEC1F0 41D13F1C EBDF3AF4 8F5AEC30 
  1D060355 1D0E0416 0414FE37 96B96FFA DEC1F041 D13F1CEB DF3AF48F 5AEC300D 
  06092A86 4886F70D 01010505 00038201 0100230C 837EF013 1CF69A36 203F6CD7 
  3E8946CE E208E2AE E984CE0B 10B9CB26 B6FFDA16 FF963EFE 53AC6C2B 799A0B04 
  4890E665 3D5F7BEE BE3DFD43 05274AE5 416EF9AC 1D7C3469 9CAA54C4 8CA1505A 
  B135FAE9 0203DD05 FDA91461 3B13F3CF 5AD0B02F F82DB025 B34425BA C6B24A43 
  FA9EC90B B602CDD5 8284C812 3F244435 D516F879 6F84DB9E 4B15966D DBC7B830 
  AF5E2E2E FA0E9075 003C3DED 93D0BF27 D5D3ACB1 0D1B7C19 84F101D5 3476F8A9 
  08D80305 48121AD1 FFFD2536 459119DA CDEAF57D 8BD2E048 A3FBFC9F CAECA895 
  3CFE9548 B3EA2B13 2A46DA8E 1FB5C4F1 98F1034E AF1DD487 87FF81EF B63CC206 
  CE7E4F15 279F6B8E 84C1D149 375D39C0 AF18
  quit
!
license udi pid CSR1000V sn 9HGGG6IZJ0U
diagnostic bootup level minimal
memory free low-watermark processor 71489
!
!
spanning-tree extend system-id
!
!
redundancy
!
!
!
!
!
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
!
! 
! 
!
!
interface Loopback0
 ip address 172.17.0.100 255.255.255.255
!
interface GigabitEthernet1
 no ip address
 shutdown
 negotiation auto
 no mop enabled
 no mop sysid
!
interface GigabitEthernet2
 no ip address
 shutdown
 negotiation auto
 no mop enabled
 no mop sysid
!
interface GigabitEthernet3
 ip address 172.16.100.2 255.255.255.0
 negotiation auto
 mpls ip
 no mop enabled
 no mop sysid
!
interface GigabitEthernet4
 no ip address
 shutdown
 negotiation auto
 no mop enabled
 no mop sysid
!
router ospf 1
 network 172.16.0.0 0.0.255.255 area 0
 network 172.17.0.0 0.0.0.255 area 0
!
router bgp 1
 bgp log-neighbor-changes
 no bgp default ipv4-unicast
 neighbor RR-Client peer-group
 neighbor RR-Client remote-as 1
 neighbor RR-Client update-source Loopback0
 neighbor RR-Client version 4
 neighbor 172.17.0.20 peer-group RR-Client
 neighbor 172.17.0.30 peer-group RR-Client
 neighbor 172.17.0.50 peer-group RR-Client
 neighbor 172.17.0.60 peer-group RR-Client
 neighbor 172.17.0.200 peer-group RR-Client
 !
 address-family ipv4
 exit-address-family
 !
 address-family vpnv4
  neighbor RR-Client send-community both
  neighbor RR-Client route-reflector-client
  neighbor 172.17.0.60 activate
  neighbor 172.17.0.200 activate
 exit-address-family
 !
 address-family l2vpn vpls
  neighbor RR-Client send-community both
  neighbor RR-Client route-reflector-client
  neighbor 172.17.0.20 activate
  neighbor 172.17.0.30 activate
  neighbor 172.17.0.50 activate
  neighbor 172.17.0.60 activate
  neighbor 172.17.0.200 activate
 exit-address-family
!
ip forward-protocol nd
no ip http server
ip http secure-server
!
!
!
!
!
!
!
!
control-plane
!
!
!
!
!
!
line con 0
 exec-timeout 0 0
 stopbits 1
line vty 0 4
 exec-timeout 0 0
 login
 length 0
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
end

AS02-ASBR01
Current configuration : 8357 bytes
!
! Last configuration change at 08:28:06 UTC Wed Aug 28 2024
!
version 17.3
service timestamps debug datetime msec
service timestamps log datetime msec
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
platform console serial
!
hostname AS02-ASBR01
!
boot-start-marker
boot-end-marker
!
!
vrf definition LAB009
 rd 9:1
 !
 address-family ipv4
  route-target export 9:1
  route-target import 9:1
 exit-address-family
!
no logging console
!
no aaa new-model
!
!
!
!
!
!
!
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
! 
! 
! 
! 
!
!
mpls ldp label
 allocate global host-routes
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
crypto pki trustpoint TP-self-signed-1486019135
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-1486019135
 revocation-check none
 rsakeypair TP-self-signed-1486019135
!
!
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030 
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363 
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934 
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305 
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720 
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030 
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D 
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520 
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE 
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC 
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188 
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7 
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191 
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44 
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201 
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85 
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500 
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905 
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B 
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8 
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C 
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B 
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678 
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB 
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0 
  D697DF7F 28
  quit
crypto pki certificate chain TP-self-signed-1486019135
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030 
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274 
  69666963 6174652D 31343836 30313931 3335301E 170D3233 30363232 31323136 
  35355A17 0D333330 36323131 32313635 355A3031 312F302D 06035504 03132649 
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 34383630 
  31393133 35308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201 
  0A028201 0100BD4C 70C8AAA9 0283A934 2E41D4C3 BBC67A82 9C1E7B85 D2583C5E 
  E5111CC2 423AAE44 8BFBA3F6 620DFFD2 CFBCC021 4EA2203B F5CCF840 37B0C3C3 
  B79FB7E0 23FF99B8 1BCDD5F1 1243CD9F 876B32D0 DEA5D1CF 81396034 BD7C1822 
  A3AEA946 E782B611 D939813C 80D46D77 FA5D2F43 F6D6B1CA BBB2ABAD D8C49A97 
  0D832E4B 468B07F7 640C47A0 8547813E 00C1672C 1D032C02 99A9DE43 91941409 
  9F5F0040 B1F0F8C0 6A93F12B 6E52952F 9DC6F0ED B95717D6 7DED856E 23452EB8 
  AAD4FCCB 3E830ED1 BB234F5A C456DFB2 691597B2 6FA3B7D8 483E127E FF87CF13 
  3C5ED12E 7DDAC5AE EF52A401 57866A47 CA91403F 4018A9EC FD266FDD 8E2D83BA 
  5F932F17 E6CB0203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF 
  301F0603 551D2304 18301680 14F7FD62 5886C776 AF17CF02 FF9C011F B635FD86 
  D7301D06 03551D0E 04160414 F7FD6258 86C776AF 17CF02FF 9C011FB6 35FD86D7 
  300D0609 2A864886 F70D0101 05050003 82010100 112B061A 80021EE5 691921D8 
  6412C7DF 8F09412D D116D944 96D6FBD7 BCA4C639 43BDD945 5AD7632C 0C61101D 
  A17F71B1 45D7BB6C A7FB17E7 601FD0D5 E48CDAAD 0175EFC2 BD4755D4 3DB15A83 
  A4C64BD2 5581FA97 1B770FDD 989364C8 BFE2943A 6FD90B14 2F4D5245 AF050570 
  F6F7B6F2 F7CC5D6C 6B2E6903 84987E39 416A1FDC 47A161C3 158B0973 09D73B18 
  9C7C8AB4 4AA651AF 1AA0A1F6 81E8B818 C844BA58 FCAD20E3 3D0652CC 4B96623F 
  7C64BC41 8AC02348 58AF161C B1E20DF8 63354C58 DCAE3DCD 7518BE63 7509A278 
  48E9B06F 6A28A950 F94F9C5B B237E7D2 BD500EE0 C4D126C2 12BB0610 FA29E365 
  65B5E2C2 B1864B71 2A157006 CB707E1C E5CFFD2A
  quit
!
license udi pid CSR1000V sn 9IVZ7D7I5CE
diagnostic bootup level minimal
memory free low-watermark processor 71489
!
!
spanning-tree extend system-id
!
!
redundancy
!
!
!
!
!
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
!
! 
! 
!
!
interface Loopback0
 ip address 172.19.0.200 255.255.255.255
!
interface pseudowire82
 encapsulation mpls
 neighbor 172.19.0.20 82
!
interface GigabitEthernet1
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 81 ethernet
  encapsulation dot1q 81
  rewrite ingress tag pop 1 symmetric
  xconnect 172.19.0.10 81 encapsulation mpls
 !
 service instance 82 ethernet
  encapsulation dot1q 82
  rewrite ingress tag pop 1 symmetric
 !
 service instance 91 ethernet
  encapsulation dot1q 91
  rewrite ingress tag pop 1 symmetric
  bridge-domain 91
 !
 service instance 101 ethernet
  encapsulation dot1q 101
  rewrite ingress tag pop 1 symmetric
  bridge-domain 101
 !
 service instance 111 ethernet
  encapsulation dot1q 111
  rewrite ingress tag pop 1 symmetric
 !
!
interface GigabitEthernet2
 no ip address
 shutdown
 negotiation auto
 no mop enabled
 no mop sysid
!
interface GigabitEthernet3
 ip address 172.18.200.2 255.255.255.0
 negotiation auto
 mpls ip
 no mop enabled
 no mop sysid
!
interface GigabitEthernet4
 no ip address
 shutdown
 negotiation auto
 no mop enabled
 no mop sysid
!
interface BDI91
 vrf forwarding LAB009
 ip address 91.0.0.2 255.255.255.0
 no mop enabled
 no mop sysid
!
interface BDI101
 ip address 101.0.0.2 255.255.255.0
 mpls ip
 no mop enabled
 no mop sysid
!
interface BDI111
 ip address 111.0.0.2 255.255.255.0
 shutdown
 no mop enabled
 no mop sysid
!
router ospf 1
 network 101.0.0.0 0.0.0.255 area 0
 network 172.18.0.0 0.0.255.255 area 0
 network 172.19.0.0 0.0.0.255 area 0
!
router bgp 2
 bgp log-neighbor-changes
 no bgp default ipv4-unicast
 no bgp default route-target filter
 neighbor 101.0.0.1 remote-as 1
 neighbor 101.0.0.1 ebgp-multihop 255
 neighbor 172.19.0.100 remote-as 2
 neighbor 172.19.0.100 update-source Loopback0
 !
 address-family ipv4
  neighbor 172.19.0.100 activate
 exit-address-family
 !
 address-family vpnv4
  neighbor 172.19.0.100 activate
  neighbor 172.19.0.100 send-community both
 exit-address-family
 !
 address-family l2vpn vpls
  neighbor 101.0.0.1 activate
  neighbor 101.0.0.1 send-community both
  neighbor 101.0.0.1 next-hop-self
  neighbor 172.19.0.100 activate
  neighbor 172.19.0.100 send-community both
  neighbor 172.19.0.100 next-hop-self
 exit-address-family
 !
 address-family ipv4 vrf LAB009
  neighbor 91.0.0.1 remote-as 1
  neighbor 91.0.0.1 activate
 exit-address-family
!
ip forward-protocol nd
no ip http server
ip http secure-server
!
!
!
!
!
l2vpn xconnect context LAB008
 member pseudowire82
 member GigabitEthernet1 service-instance 82 
!
!
!
!
control-plane
!
!
!
!
!
!
line con 0
 exec-timeout 0 0
 stopbits 1
line vty 0
 exec-timeout 0 0
 login
 transport input ssh
line vty 1
 exec-timeout 0 0
 login
 length 0
 transport input ssh
line vty 2 4
 exec-timeout 0 0
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
end

##################################################################################

AS02-CE01
Current configuration : 3768 bytes
!
version 15.9
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname AS02-CE01
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
ip vrf 2111
 rd 21:11
!
ip vrf 2181
 rd 21:81
!
ip vrf 2191
 rd 21:91
!
!
!
!
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
redundancy
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/1.2181
 encapsulation dot1Q 2181
 ip vrf forwarding 2181
 ip address 10.21.8.1 255.0.0.0
!
interface GigabitEthernet0/2
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/3
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/3.2191
 encapsulation dot1Q 2191
 ip vrf forwarding 2191
 ip address 10.21.9.1 255.255.255.0
!
interface GigabitEthernet0/4
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/4.2111
 encapsulation dot1Q 2111
 ip vrf forwarding 2111
 ip address 10.21.11.1 255.0.0.0
!
interface GigabitEthernet0/5
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/6
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/7
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
ip route vrf 2191 0.0.0.0 0.0.0.0 10.21.9.2
!
ipv6 ioam timestamp
!
!
!
control-plane
!
banner exec <
>
!
line con 0
 exec-timeout 0 0
line aux 0
line vty 0 4
 exec-timeout 0 0
 login
 transport input none
!
no scheduler allocate
!
end

##################################################################################

AS02-CE02
Current configuration : 3196 bytes
!
version 15.9
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname AS02-CE02
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
ip vrf 2211
 rd 22:11
!
ip vrf 2281
 rd 22:81
!
!
!
!
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
redundancy
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/1.2281
 encapsulation dot1Q 2281
 ip vrf forwarding 2281
 ip address 10.22.8.1 255.0.0.0
!
interface GigabitEthernet0/2
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/3
 no ip address
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/3.2211
 encapsulation dot1Q 2211
 ip vrf forwarding 2211
 ip address 10.22.10.1 255.0.0.0
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 ioam timestamp
!
!
!
control-plane
!
banner exec <
>
!
line con 0
 exec-timeout 0 0
line aux 0
line vty 0 4
 exec-timeout 0 0
 login
 transport input none
!
no scheduler allocate
!
end

AS02-P01
Current configuration : 3151 bytes
!
version 15.9
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname AS02-P01
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
redundancy
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 172.19.0.1 255.255.255.255
!
interface GigabitEthernet0/0
 ip address 172.18.0.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls ip
!
interface GigabitEthernet0/1
 ip address 172.18.3.2 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls ip
!
interface GigabitEthernet0/2
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/3
 ip address 172.18.200.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls ip
!
router ospf 1
 network 172.18.0.0 0.0.255.255 area 0
 network 172.19.0.0 0.0.0.255 area 0
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 ioam timestamp
!
!
!
control-plane
!
banner exec <
>
!
line con 0
 exec-timeout 0 0
line aux 0
line vty 0 4
 exec-timeout 0 0
 login
 transport input none
!
no scheduler allocate
!
end

##################################################################################

AS02-P02
Current configuration : 3151 bytes
!
version 15.9
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname AS02-P02
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
redundancy
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 172.19.0.2 255.255.255.255
!
interface GigabitEthernet0/0
 ip address 172.18.0.2 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls ip
!
interface GigabitEthernet0/1
 ip address 172.18.1.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls ip
!
interface GigabitEthernet0/2
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
interface GigabitEthernet0/3
 ip address 172.18.100.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls ip
!
router ospf 1
 network 172.18.0.0 0.0.255.255 area 0
 network 172.19.0.0 0.0.0.255 area 0
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 ioam timestamp
!
!
!
control-plane
!
banner exec <
>
!
line con 0
 exec-timeout 0 0
line aux 0
line vty 0 4
 exec-timeout 0 0
 login
 transport input none
!
no scheduler allocate
!
end

##################################################################################

AS02-P03
Current configuration : 3150 bytes
!
version 15.9
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname AS02-P03
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
redundancy
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 172.19.0.3 255.255.255.255
!
interface GigabitEthernet0/0
 ip address 172.18.2.2 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls ip
!
interface GigabitEthernet0/1
 ip address 172.18.3.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls ip
!
interface GigabitEthernet0/2
 ip address 172.18.10.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls ip
!
interface GigabitEthernet0/3
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
router ospf 1
 network 172.18.0.0 0.0.255.255 area 0
 network 172.19.0.0 0.0.0.255 area 0
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 ioam timestamp
!
!
!
control-plane
!
banner exec <
>
!
line con 0
 exec-timeout 0 0
line aux 0
line vty 0 4
 exec-timeout 0 0
 login
 transport input none
!
no scheduler allocate
!
end

##################################################################################

AS02-P04
Current configuration : 3150 bytes
!
version 15.9
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname AS02-P04
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
ip cef
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
redundancy
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 172.19.0.4 255.255.255.255
!
interface GigabitEthernet0/0
 ip address 172.18.2.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls ip
!
interface GigabitEthernet0/1
 ip address 172.18.1.2 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls ip
!
interface GigabitEthernet0/2
 ip address 172.18.20.1 255.255.255.0
 duplex auto
 speed auto
 media-type rj45
 mpls ip
!
interface GigabitEthernet0/3
 no ip address
 shutdown
 duplex auto
 speed auto
 media-type rj45
!
router ospf 1
 network 172.18.0.0 0.0.255.255 area 0
 network 172.19.0.0 0.0.0.255 area 0
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 ioam timestamp
!
!
!
control-plane
!
banner exec <
>
!
line con 0
 exec-timeout 0 0
line aux 0
line vty 0 4
 exec-timeout 0 0
 login
 transport input none
!
no scheduler allocate
!
end

##################################################################################

AS02-PE01
Current configuration : 7222 bytes
!
! Last configuration change at 07:57:12 UTC Wed Aug 28 2024
!
version 17.3
service timestamps debug datetime msec
service timestamps log datetime msec
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
platform console serial
!
hostname AS02-PE01
!
boot-start-marker
boot-end-marker
!
!
vrf definition LAB009
 rd 9:1
 !
 address-family ipv4
  route-target export 9:1
  route-target import 9:1
 exit-address-family
!
no logging console
!
no aaa new-model
!
!
!
!
!
!
!
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
! 
! 
! 
! 
!
!
mpls ldp label
 allocate global host-routes
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
crypto pki trustpoint TP-self-signed-568474736
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-568474736
 revocation-check none
 rsakeypair TP-self-signed-568474736
!
!
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030 
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363 
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934 
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305 
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720 
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030 
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D 
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520 
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE 
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC 
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188 
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7 
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191 
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44 
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201 
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85 
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500 
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905 
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B 
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8 
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C 
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B 
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678 
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB 
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0 
  D697DF7F 28
  quit
crypto pki certificate chain TP-self-signed-568474736
 certificate self-signed 01
  3082032E 30820216 A0030201 02020101 300D0609 2A864886 F70D0101 05050030 
  30312E30 2C060355 04031325 494F532D 53656C66 2D536967 6E65642D 43657274 
  69666963 6174652D 35363834 37343733 36301E17 0D323330 36323231 32313730 
  355A170D 33333036 32313132 31373035 5A303031 2E302C06 03550403 1325494F 
  532D5365 6C662D53 69676E65 642D4365 72746966 69636174 652D3536 38343734 
  37333630 82012230 0D06092A 864886F7 0D010101 05000382 010F0030 82010A02 
  82010100 CA2BA753 47E6022D EF8CE5DD EFB232B7 364B116B C457DAE3 9F8D19F7 
  D21A8CD5 B9AFF676 D79BF15A A33D5488 B6E0C4FC 26C08DE9 DD2D086D F3A83F05 
  8993DBD8 C4007618 6D6BEF8B 102969F1 D7FDD0FC B707B493 66CD520B E3E56C18 
  8252EDB3 AE82659D 89A0079F 476D5B6C 18285809 E49002E6 F5D4CECF 51C272B0 
  5499B115 ECD521FF 4C21D985 0BBB2EA6 8975D6A6 4E1D7AE2 E2C04FBD B5D60106 
  C63395F9 CE6ADADF D6C50D15 2EE68BEA 4E619DA5 B1A08011 E2E8D62D D5DD3C5D 
  0706A9C9 1D5AD94D 014495EA 725C0E8E 8EDA92C4 66A3CF01 E1175A16 27CC3AB8 
  EC1F7971 4BF59949 CDD98220 D31FD853 B749F507 55765F1A 89495923 42F1B54D 
  966CC0EF 02030100 01A35330 51300F06 03551D13 0101FF04 05300301 01FF301F 
  0603551D 23041830 168014A2 9BEA0D9F 6BE26B8B A5EBEDAB 98C9A57B 99660830 
  1D060355 1D0E0416 0414A29B EA0D9F6B E26B8BA5 EBEDAB98 C9A57B99 6608300D 
  06092A86 4886F70D 01010505 00038201 010072CB 6E26D97A E920D3CC FD02EA20 
  D4AA26EB 13952BE3 BA26A6FF DA057589 73B0F80B 8D57D744 A2427297 7B6F7E97 
  A46F3842 2E164C46 F7BBB9DC 96B681C9 32CA8CE9 A6624593 754EE987 42446091 
  7B8AEC37 E8005CB4 F159A11D C3C9B383 7AC2ED01 17AD67B0 2D5EBA79 01DE0768 
  9E1CD987 EB5B6089 D50A9A54 CAD8A333 7B68B46F 427918C1 A47E6E63 CED8090D 
  7F661DA6 80B08381 86BB273E 9B8EAD92 0AD96C75 2B852BF8 CC9156A4 38BDE092 
  89F6A9A3 352DF59F B14576EA C9423F92 86393EE5 23F2D43E 98FA4142 2E04BB70 
  9196E53B F985EA84 59C39079 9285CB83 10FB389B FE978495 A3BA5515 95931FCB 
  D4DB3BB5 1B52A793 BB5BC1E4 A0AC8C4E AF56
  quit
!
license udi pid CSR1000V sn 98CD4L3VY7B
diagnostic bootup level minimal
memory free low-watermark processor 71489
!
!
spanning-tree extend system-id
!
!
redundancy
!
!
!
!
!
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
!
! 
! 
!
!
interface Loopback0
 ip address 172.19.0.10 255.255.255.255
!
interface GigabitEthernet1
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 2181 ethernet
  encapsulation dot1q 2181
  rewrite ingress tag pop 1 symmetric
  xconnect 172.19.0.200 81 encapsulation mpls
 !
!
interface GigabitEthernet2
 ip address 172.18.10.2 255.255.255.0
 negotiation auto
 mpls ip
 no mop enabled
 no mop sysid
!
interface GigabitEthernet3
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 2191 ethernet
  encapsulation dot1q 2191
  rewrite ingress tag pop 1 symmetric
  bridge-domain 91
 !
!
interface GigabitEthernet4
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 2111 ethernet
  encapsulation dot1q 2111
  rewrite ingress tag pop 1 symmetric
 !
!
interface BDI91
 vrf forwarding LAB009
 ip address 10.21.9.2 255.255.255.0
 no mop enabled
 no mop sysid
!
router ospf 1
 network 172.18.0.0 0.0.255.255 area 0
 network 172.19.0.0 0.0.0.255 area 0
!
router bgp 2
 bgp log-neighbor-changes
 neighbor 172.19.0.100 remote-as 2
 neighbor 172.19.0.100 update-source Loopback0
 !
 address-family vpnv4
  neighbor 172.19.0.100 activate
  neighbor 172.19.0.100 send-community both
 exit-address-family
 !
 address-family ipv4 vrf LAB009
  network 10.21.9.0 mask 255.255.255.0
 exit-address-family
!
ip forward-protocol nd
no ip http server
ip http secure-server
!
!
!
!
!
!
!
!
control-plane
!
!
!
!
!
!
line con 0
 exec-timeout 0 0
 stopbits 1
line vty 0
 exec-timeout 0 0
 login
 transport input ssh
line vty 1
 exec-timeout 0 0
 login
 length 0
 transport input ssh
line vty 2 4
 exec-timeout 0 0
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
end

##################################################################################

AS02-PE02
Current configuration : 7191 bytes
!
! Last configuration change at 08:32:28 UTC Wed Aug 28 2024
!
version 17.3
service timestamps debug datetime msec
service timestamps log datetime msec
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
platform console serial
!
hostname AS02-PE02
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
!
!
!
!
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
! 
! 
! 
! 
!
!
mpls ldp label
 allocate global host-routes
mpls ldp discovery targeted-hello accept
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
crypto pki trustpoint TP-self-signed-1340914802
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-1340914802
 revocation-check none
 rsakeypair TP-self-signed-1340914802
!
!
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030 
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363 
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934 
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305 
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720 
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030 
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D 
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520 
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE 
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC 
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188 
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7 
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191 
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44 
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201 
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85 
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500 
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905 
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B 
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8 
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C 
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B 
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678 
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB 
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0 
  D697DF7F 28
  quit
crypto pki certificate chain TP-self-signed-1340914802
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030 
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274 
  69666963 6174652D 31333430 39313438 3032301E 170D3233 30363233 31303539 
  35305A17 0D333330 36323231 30353935 305A3031 312F302D 06035504 03132649 
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 33343039 
  31343830 32308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201 
  0A028201 0100B8C7 BD5915DF A928E472 CEC1CE2B 191B5463 AC85A07F 15DEA8A9 
  71B798A5 C051A9DE 2BED2E44 9692D007 16F84D82 D0B47F2C 22DE0F89 D2B8FAE0 
  016B4C0B 05A95BB8 438CCF40 4DA940B9 2619D04A 5ED539DD EAA0EA92 25CDFB13 
  6AB6085E 65B38637 0DE2788C 47819AA6 D1F9E13A 3906CF58 63B25670 60C14084 
  97532CC7 58A72B25 E34D4B10 B8C75631 DB972010 5462195D 2F1EBE49 C0206E58 
  0C813549 72E57548 135C7777 6C7D7C5E 778E7BCC 3E0F2306 BDAFDE5B 00949149 
  1A7FD49F 7AAED7D4 C47E54A3 C130C978 F6748122 DA45EAA8 791C9B15 F3086D77 
  8151F677 A8920FC6 EC6535B9 E77A2220 C685994D C7CA92C8 D343ADD2 F6D8BB82 
  41EB11A4 D0150203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF 
  301F0603 551D2304 18301680 140AA13F 6C2E5A23 EC29CA40 ED112618 34264838 
  09301D06 03551D0E 04160414 0AA13F6C 2E5A23EC 29CA40ED 11261834 26483809 
  300D0609 2A864886 F70D0101 05050003 82010100 1224C316 B9D6984B 8200331B 
  137334FD B87715A6 031833F5 701F004B BDFC4A46 7AACC116 F76C4A8F 6C224EA1 
  98DBC457 291F4F39 7B1E42C0 F19AED5A 697D3582 8F6DD3D5 D8DDFEA9 2EBEADBF 
  A6CB634D A4CD1B61 BC16C243 8661968A B50574EB D7A6ED8D 54BC02F3 F5542890 
  DFA5D87B F6BE4C01 458CD1A6 CE5F7DE3 566DFCB1 E1EDC413 367CB57C 8BCB95F9 
  92887D48 92971FB6 FE58F80E B96DF70B 36C7D17D 13ABDC93 DFD7F28E DBC1F4D9 
  46A7FC64 E39138CE 844C0DB4 75403D36 4A19DADA D94FE4C6 AE57EC9B 896B0FA2 
  70DF938F 02253F26 679E0186 DC5284B9 8C7950FD 3C49AA8B 9CF4C6C2 48332460 
  F0C3B643 5D9E6A18 AE7148EE FFF19243 57355447
  quit
!
license udi pid CSR1000V sn 9V2EW8DTVAS
diagnostic bootup level minimal
memory free low-watermark processor 71489
!
!
spanning-tree extend system-id
!
!
redundancy
!
!
!
!
!
!
!
l2 pseudowire routing
 terminating-pe tie-breaker
l2 vfi LAB010 autodiscovery 
 vpn id 101
 bridge-domain 101
 vpls-id 10:1
 rd 10:1
 route-target export 10:1
 route-target import 10:1
 no auto-route-target
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
!
! 
! 
!
!
interface Loopback0
 ip address 172.19.0.20 255.255.255.255
!
interface pseudowire82
 encapsulation mpls
 neighbor 172.19.0.200 82
!
interface GigabitEthernet1
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 2281 ethernet
  encapsulation dot1q 2281
  rewrite ingress tag pop 1 symmetric
 !
!
interface GigabitEthernet2
 ip address 172.18.20.2 255.255.255.0
 negotiation auto
 mpls ip
 no mop enabled
 no mop sysid
!
interface GigabitEthernet3
 no ip address
 negotiation auto
 no mop enabled
 no mop sysid
 service instance 2211 ethernet
  encapsulation dot1q 2211
  rewrite ingress tag pop 1 symmetric
  bridge-domain 101
 !
!
interface GigabitEthernet4
 no ip address
 shutdown
 negotiation auto
 no mop enabled
 no mop sysid
!
router ospf 1
 network 172.18.0.0 0.0.255.255 area 0
 network 172.19.0.0 0.0.0.255 area 0
!
router bgp 2
 bgp log-neighbor-changes
 neighbor 172.19.0.100 remote-as 2
 neighbor 172.19.0.100 update-source Loopback0
 !
 address-family l2vpn vpls
  neighbor 172.19.0.100 activate
  neighbor 172.19.0.100 send-community both
 exit-address-family
!
ip forward-protocol nd
no ip http server
ip http secure-server
!
!
!
!
!
l2vpn xconnect context LAB008
 member pseudowire82
 member GigabitEthernet1 service-instance 2281 
!
!
!
!
control-plane
!
!
!
!
!
!
line con 0
 exec-timeout 0 0
 stopbits 1
line vty 0
 exec-timeout 0 0
 login
 transport input ssh
line vty 1
 exec-timeout 0 0
 login
 length 0
 transport input ssh
line vty 2 4
 exec-timeout 0 0
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
end

##################################################################################

AS02-RR01
Current configuration : 7099 bytes
!
! Last configuration change at 08:30:11 UTC Wed Aug 28 2024
!
version 17.3
service timestamps debug datetime msec
service timestamps log datetime msec
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
platform console serial
!
hostname AS02-RR01
!
boot-start-marker
boot-end-marker
!
!
no logging console
!
no aaa new-model
!
!
!
!
!
!
!
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
! 
! 
! 
! 
!
!
mpls ldp label
 allocate global host-routes
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
crypto pki trustpoint TP-self-signed-1939541390
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-1939541390
 revocation-check none
 rsakeypair TP-self-signed-1939541390
!
!
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030 
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363 
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934 
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305 
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720 
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030 
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D 
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520 
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE 
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC 
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188 
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7 
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191 
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44 
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201 
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85 
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500 
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905 
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B 
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8 
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C 
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B 
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678 
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB 
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0 
  D697DF7F 28
  quit
crypto pki certificate chain TP-self-signed-1939541390
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030 
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274 
  69666963 6174652D 31393339 35343133 3930301E 170D3233 30363236 31353136 
  32315A17 0D333330 36323531 35313632 315A3031 312F302D 06035504 03132649 
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 39333935 
  34313339 30308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201 
  0A028201 0100B91F E5898C1E F5CA58FC 606CF4A7 AA0A7554 AEECC2F5 B3E7545F 
  D0528AC6 F13253FF 5D94C9C3 67245F0F BEFE05AE 0DF23C90 F44A21AC 867C3971 
  E6553A83 5B0B7FB3 44AB69E4 E5754480 8FA42335 A10955FA 4AD30030 66DB6822 
  55CC85A5 305445D2 92006020 0870FC8B 2ACEB519 AEE7988F E1495A62 542303C8 
  6EAC66D1 9AC32180 2CF90706 E771FB27 65C3A804 47A4AE8B 7249C930 ACD9A48E 
  574602C3 26E6014A 1218EE08 D253F5A0 28BA5952 F5507FA1 B6A8C4C0 3EF8E2F2 
  1E758FC9 57BE5692 64F09A7E 9595406B 09D6F5D9 53EB1935 FEEA4D98 CABE88BE 
  B9FFBE51 BD0D3F45 6DFA4308 75B214F0 AF1A9C9D 9E98998F 687035AC 8277C786 
  61D2F1DE 27C70203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF 
  301F0603 551D2304 18301680 149A28EE EB61CF5E 7D25BE39 32060ADE E113D4CB 
  B6301D06 03551D0E 04160414 9A28EEEB 61CF5E7D 25BE3932 060ADEE1 13D4CBB6 
  300D0609 2A864886 F70D0101 05050003 82010100 86513B28 0F6359FC 6B4E5454 
  BCFA46EB CDA5D1B3 E973F7A3 EF8C437C 7D4EFBB0 FD99943D 7888A655 824DD981 
  81117B26 A3EB6250 81F506B5 EFA0946B 16F07982 0444B24E 98D79674 3D5B8256 
  3F748AE1 E55F3FCC 1616A7D4 D155CCB2 A5464900 5BE3C7E0 A730111D 8F765BA8 
  C7ECC32B F91F8EB3 681AB57E E95B8640 0D542E83 D795D20A F4866259 C91AA491 
  8EFB74E3 933C3D07 3447336F 62D2E82A 241DF4B4 31255A03 DA5D3FB9 3CDAEAA0 
  25D44687 112AB9CB 366218C1 8AF62E0A 341A7975 6D7D5350 ABD5F2BF 094A0872 
  19C12CAB 13968DF7 B1262B83 2E599E93 CC3552B2 D04AEF93 D62A89FC C951E0A9 
  66EA0244 F0BB4F5B 79B86A44 A5EBC793 DA7E4E82
  quit
!
license udi pid CSR1000V sn 92KZBJLPQ3X
diagnostic bootup level minimal
memory free low-watermark processor 71489
!
!
spanning-tree extend system-id
!
!
redundancy
!
!
!
!
!
!
!
! 
!
!
!
!
!
!
!
!
!
!
!
!
!
! 
! 
!
!
interface Loopback0
 ip address 172.19.0.100 255.255.255.255
!
interface GigabitEthernet1
 no ip address
 shutdown
 negotiation auto
 no mop enabled
 no mop sysid
!
interface GigabitEthernet2
 no ip address
 shutdown
 negotiation auto
 no mop enabled
 no mop sysid
!
interface GigabitEthernet3
 ip address 172.18.100.2 255.255.255.0
 negotiation auto
 mpls ip
 no mop enabled
 no mop sysid
!
interface GigabitEthernet4
 no ip address
 shutdown
 negotiation auto
 no mop enabled
 no mop sysid
!
router ospf 1
 network 172.18.0.0 0.0.255.255 area 0
 network 172.19.0.0 0.0.0.255 area 0
!
router bgp 2
 bgp log-neighbor-changes
 no bgp default ipv4-unicast
 neighbor RR-Client peer-group
 neighbor RR-Client remote-as 2
 neighbor RR-Client update-source Loopback0
 neighbor RR-Client version 4
 neighbor 172.19.0.10 peer-group RR-Client
 neighbor 172.19.0.20 peer-group RR-Client
 neighbor 172.19.0.200 peer-group RR-Client
 !
 address-family ipv4
 exit-address-family
 !
 address-family vpnv4
  neighbor RR-Client send-community both
  neighbor RR-Client route-reflector-client
  neighbor 172.19.0.10 activate
  neighbor 172.19.0.200 activate
 exit-address-family
 !
 address-family l2vpn vpls
  neighbor RR-Client send-community both
  neighbor RR-Client route-reflector-client
  neighbor 172.19.0.20 activate
  neighbor 172.19.0.200 activate
 exit-address-family
!
ip forward-protocol nd
no ip http server
ip http secure-server
!
!
!
!
!
!
!
!
control-plane
!
!
!
!
!
!
line con 0
 exec-timeout 0 0
 stopbits 1
line vty 0
 exec-timeout 0 0
 login
 transport input ssh
line vty 1
 exec-timeout 0 0
 login
 length 0
 transport input ssh
line vty 2 4
 exec-timeout 0 0
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
end